	CAP PILOT FLIGHT EVALUATION QUESTIONNAIRE

	MEMBER’S NAME & GRADE
	CAPID
	AIRCRAFT MAKE & MODEL

	
	
	 C-182T  N290CP

	

	CHECK PILOT NAME & GRADE
	CAPID
	SCORE
	DATE

	
	
	
	


Complete this open book questionnaire using the Flight Manual/Pilot's Operating Handbook/STC. If a question or part of a question is not applicable, write in NA. The check pilot will review and grade the questionnaire. Minimum passing score is 80% corrected to 100%. The completed, scored, and corrected questionnaire will be filed in the pilot's flight records.
1. Total fuel capacity 92 (pg 1-6)	gal.  Usable fuel 87 (pg 1-6)	gal.	Location Wing and Belly	.
2. Number of fuel drains_13 (7-44) 	.	Fuel color Blue/Green (1-6)	.
3. Today’s average fuel burn is estimated to be 14	GPH; providing 6.2	hours of endurance.
4. Oil capacity is 8 (pg 1-7)	quarts.  Minimum for takeoff is 4 (pg 4-9)	quarts.
5. Max takeoff weight 3100 (pg 1-8)	.	Max Landing weight 2950 (pg 1-8)	.
6. [image: ]Maximum RPM and MP for takeoff are 2400 (pg 2-7) Green Arc and full (pg 4-18)	in/Hg.
7. C182/C206/GA8 – Max climb power	MP full (4-19) RPM 2400 (pg 4-19)
8. White ARC 41-100 (pg 2-5) KIAS Range.  Green ARC 51-140 (pg 2-5)	KIAS Range.
9. Gliding distance @ 3,500ft AGL, Max Weight, Zero Wind 5  (pg 3-36)	.
10. This plane operates on a 28 (7-49)- volts electrical system. Main battery 24 (7-49) volts. 
11. Magnetos are checked at 1800	RPM. RPM drop should not exceed 175	RPM (pg 4-16)
12. Useful load for today’s flight is 1186 max	.
13. Takeoff & Landing distance for today’s flight is	T/O: 	_ Landing: 	.
14. Today’s Density Altitude is 	.
Provide the following airspeeds in KIAS at maximum gross weight?
	Va (maneuvering speed)
	110 (pg 2-4)
	
	Vx (best angle of climb, sea level)
	65 (pg 4-3)

	Vso (stall, landing config) Forward CC
	41 (pg 5-14)
	
	Vy (best rate of climb, sea level)
	80 (pg 4-3)

	Vs1 (stall, cruise config) Forward CC
	51 (pg 5-14)
	
	Best glide Speed
	75 (pg 3-5)

	Vne (never exceed speed)
	175 (pg 2-4)
	
	  
	


Complete the BOLD FACE memory items for the following emergencies.
· Engine failure immediately after takeoff.
1. Airspeed – 75 KIAS (flaps UP) 70 (flaps DOWN)
2. Mixture – IDLE CUT OFF
3. Fuel Selector Valve – OFF
4. MAGNETOS Switch – OFF
5. STBY BATT Switch -- OFF
6. Wing Flaps – AS REQUIRED (40 RECOMMENDED)
7. Master Switch – OFF
8. Cabin Door – UNLATCH
9. Land – STRAIGHT AHEAD
· Engine fire during start.
1. MAGNETOS Switch - START (continue cranking to start the engine) 

IF ENGINE STARTS 
2. Power - 1800 RPM (for a few minutes) 
3. Engine - SHUTDOWN (inspect for damage) 
IF ENGINE FAILS TO START 
2. Throttle Control - FULL (push full in) 
3. Mixture Control - IDLE CUTOFF (pull full out) 
4. MAGNETOS Switch - START (continue cranking) 
5. FUEL SELECTOR Valve - PUSH DOWN and ROTATE to OFF 
6. FUEL PUMP Switch - OFF 
7. MAGNETOS Switch - OFF 
8. STBY BATT Switch - OFF 
9. MASTER Switch (ALT and BAT) - OFF 
10. Engine - SECURE 
11. Parking Brake - RELEASE 
12. Fire Extinguisher - OBTAIN (have ground attendants obtain if not installed) 
13. Airplane - EVACUATE 
14. Fire - EXTINGUISH (using fire extinguisher, wool blanket, or dirt) 
15. Fire Damage - INSPECT (repair or replace damaged components and/or wiring before conducting another flight)
· Engine failure during flight (Restart).
1. Airspeed – 75 KIAS (flaps UP) 
2. Mixture – RICH
3. Fuel Selector Valve – BOTH
4. Fuel pump Switch - ON
5. MAGNETOS Switch - BOTH

· Autopilot or Electrical Trim Failure (if applicable) otherwise Engine Fire during flight
1. Mixture Control - IDLE CUTOFF (pull full out) 
2. FUEL SELECTOR Valve - PUSH DOWN and ROTATE to OFF 
3. FUEL PUMP Switch - OFF 
4. MASTER Switch (ALT and BAT) - OFF 
5. Cabin Vents - OPEN (as needed) 
6. CABIN HT and CABIN AIR Control Knobs - OFF (push full in) 
7. Airspeed - 100 KIAS (If fire is not extinguished, increase glide speed to find an airspeed, within airspeed limitations, which will provide an incombustible mixture) 
8. Forced Landing - EXECUTE (refer to EMERGENCY LANDING WITHOUT ENGINE POWER
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